# Welcome to Trainer 1149!

## Learn how Boundary Scan works

- Look inside Boundary Scan cells
- Walk through TAP controller states
- Play with Boundary Scan controller
- Inject faults and observe their effects
- Connect your hardware and control it
- Build your programs and execute SVFs
- Create your own board and simulate it
- Import your BSDL files (see www.bsdl.info)

## Quick start with Trainer 1149

### About this help

This help is located in Text Editor tab panel. It can always be seen by clicking on this tab panel:

### General info

Now you are working with "example_project" project. To switch to another project select File->Open menu.

### Working modes

There are three working modes supported by Trainer 1149:

- Project Mode - allows you to view/organize your project items, create or import new files
- Debug Mode - is used to perform Boundary Scan operations on currently opened netlist: select instructions, perform scan, define test vectors, observe diagnostic results, etc
- Board Edit Mode - intended to create/edit your own netlists

To change the working mode select appropriate item in the Mode menu. Another way is two use special toolbar buttons:

Your should start your work with Project Mode to choose the netlist first.

#### Opening netlist

As a first step you should choose some netlist to work with. Expand the Project Explorer tree to Netlists group and choose one of the available netlists:

Netlists are stored in files with .NL extension.

To open netlist - just double click on it. Shortly after, the Boundary Scan part of the board become visualized in the Board panel.

### Board

After netlist is opened the Boundary Scan part of board become visualized. You can see BS chips, BS cells, Instruction and Bypass registers, IDCODE/USERCODE registers (if present), connections between chips, external I/O etc.

If the description of internal logic is present in the board descirption the full simulation become available.

The colors of signal lines will represent a current values of signals.
You can also click on input pins to change the input values.

### Performing BS operations

To perform BS-related operations you need to swicth to the Debug Mode.

Test Constructor panel will appear in the left:
Here you can specify instructions for each of BS chips and shifting values (test patterns). After that, press the Run button to perform scan (you can also perform Scan IR and Scan DR operations separately by pressing corresponding buttons).

Also you can select instructions and input scan values directly on the board by mouse clicks:

The results of scans are displayed in the Diagnostic Results panel in the bottom:

### Working with TAP controller

You can work with Boundary Scan by accessing TAP controller directly.

Go to Window->Tap state diagram menu (or press appropriate button in the toolbar). TAP state diagram become visible.
Click TDI and TMS buttons to change input signals. After TCK button is pressed the clock cycle will be generated and controller might change its state. Pressing TCK button while Shift is holded down will generate clock edges.

You can speed-up your work with TAP controller by clicking on hightlighted states. In the last case the software will generate needed sequence of TCK/TMS signals automatically.

You can see how signals and TAP state changes in the Signal Watcher:

### Injecting faults

The following fault types can be injected:

- Opens (stuck-at model)
- Shorts (Wired-OR, Wired-AND or Dominant models)

To inject fault choose Training->Inject Fault... menu item. In the special dialog you can select fault type and location or inject a random fault.

After that you can try to identify fault by using means of Bounary Scan. To check your guess, use Training->Check Fault menu item.

To remove the injected fault from the board use Training->Remove Injected Fault menu item.

## Further info

Certainly you can do much more with Trainer 1149 than it was described above.

You can ask for additional information at http://www.testonica.com.

Copyright © Testonica Lab. All rights reserved.